**Instructions for wallpapering**

Before open the package of rolls, make sure that you have received the Wallpaper of the required article; the batch number is the same on all rolls. Check the appearance of the rolls before cutting them into the canvas. All non-conformities must be identified prior before the work with the rolls. Be sure to keep the label attached to the roll until the work is finished and within 2 days after.

**Wall preparation**

The walls should be flat, smooth, dry, durable and clean, without peeling paint, grease, old Wallpaper glue and mold. Various defects of the walls, not removed during preparation, will be visible after the wallpapering and can affect the quality. The surface should not be covered with varnish, have non-absorbent areas and grease stains. Painted surfaces must be washed from dirt and salt stains or deposits. It is impossible to paste over the surfaces covered with fresh plaster without preliminary drying and a primer. All walls must be primed. Wallpapering should be done at 20-25 °C room temperature.

**Preparation of canvas**

Cut the roll on the number of lanes, which allows to cut the height of the ceiling of the room with a plot of the fit of the pattern (see label) and allowance (for alignment) at 5 cm from the top and bottom of each strip. For wallcoverings with a picture fit, combine the next strip with the previous strip (already cut off) to a match of the picture and only then cut it off from the main roll. Number each canvas in the order of cutting from the roll. Wallpaper should be glued in the same sequence in which they are cut off from the roll.

Before gluing the first canvas, draw a vertical line (using a plumb) from which the Wallpaper will be pasted. Apply a uniform layer of glue to the surface of the wall or Wallpaper in an amount as specified in the instructions. Make sure that the glue is evenly covers all the canvas, especially the edges. Put canvas to the wall. The top and bottom of the intended edge of it remained 3-5 cm. Smoothing should be done with a soft sponge or wallpaper brush from top to bottom. Protruding from the top and bottom edges are cut with a very sharp knife. Put the next canvas to the previous one, if necessary, combining the pattern. You need to inflict a uniform layer of glue on the wall.

Follow the instructions carefully, as the manufacturer does not consider the claim if the wallpaper gluing technique is incorrect. Keep the labels until the end of the work. Without rolls labels no claims are considered. If necessary, it will also help with new order, if you make a mistake in the calculation.

The quality and aesthetic appearance of the wallpapered wall are largely determined by the skill and qualifications of the maintenance men.

The supplier shall not be liable for defects arising during the installation process, as well as for labor costs associated with the pasting of defective Wallpaper and Wallpaper pasted in violation of this instruction. Claims for difference in shades or the difference in the numbers of the received materials, after the cutting rolls into canvas will not be accepted. After gluing two or three canvas, be sure to check them for any defects and only then continue. Claims for damages will not be accepted if more than one roll is used. If you find a defect, you should immediately stop and contact the seller. Gluing the entire volume of Wallpaper confirms that the product is accepted and satisfied with the quality.

And again: pay attention – defective goods are returned with all the labels only.